Okay,

this small patch would update

U-Boot (+config)
W-Load
Kernel
Initrd

and some environment settings


You'll find a file called 'VERSION_CONFIG' in FirmwareInstall/ Directory; 
(Use a text editor that saves with unix-line endings; such as notepad++ or notepad2 .. or vi .. etc)

In this configuration file you can currently switch the 'to patch' versions of w-load and the kernel



The file you're choosing has to exist in the FirmwareInstall folder (the installation routine will check for existance; so a typo wont break anything)





Preconfigured in this release is 
Wload: w-load_DDR2_700M_800M_8bit_2_0090003.bin

Kernel & initrd from 1.2.2 (7_inch_VIA8650-Uberoid_WM8650_2.2_v1.2.2_NL_20110409-HcH)






If you have Any questions - Feel free and ASK! 



